 TWD Scientific, LLC

10555 86th Avenue

Pleasant Prairie, WI 53158

|  |  |
| --- | --- |
| **888.323.3585 TEL** | **262.605.3262 FAX** |

**www.twdtradewinds.com**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **PART #:** | **REF #:** | **DESCRIPTION:** | | **LOT #:** |
| **DF8088S** | **84011600** | **DISPOSABLE POLYSTYRENE STERILE BLUE FORCEPS WITH BLUNT TIP. FORCEPS ARE INDIVIDUALLY PEEL-PACKED.** | | **358147** |
| **STERILIZATION DATE: 2024-08-26 (YYYY-MM-DD)** | | | **EXPIRATION DATE: 2029-07-31 (YYYY-MM-DD)** | |

**CERTIFICATE OF STERILIZATION**

The validation and routine control of the sterilization process are carried out in accordance with the following standards:

EN ISO 11135: 2014 Sterilization of health care products – Ethylene oxide – Part 1: Requirements for development, validation and routine control of a sterilizations process for medical devices

EN 556-1: 2001 Sterilization of medical devices – Requirements for medical devices to be designated “Sterile” – Part 1: Requirements for terminally sterilized medical devices

EN ISO 10993-7: 2008 Biological evaluation of medical devices – Part 7: Ethylene oxide sterilization residuals

Routine control: The criteria for product release from sterilization

- Conformity with the specified physical parameters for the sterilization cycle

- No growth of the biological indicators

Provided appropriately stored, products remain sterile for at least 5 years from the sterilization date.

**CERTIFICATE OF CONFORMITY**

Has been developed, manufactured, inspected and sterilized in accordance with the requirements of:

ISO 13485:2016: Quality systems – Medical devices.

EN ISO 13485:2016: Quality systems – Medical devices.

EN ISO 11135-2014 Sterilization of health care products – Ethylene oxide – Part 1: Requirements for

development, validation and routine control of a sterilizations process for medical

devices

EN 556-1, 2001: Sterilization of medical devices –

Requirements for medical devices to be designated “Sterile”

Part 1: Requirement for terminally sterilized medical devices